

Skip placement checklist

Complete this checklist each time you deliver a skip, bin or container.

# Assess the location

Ensure the skip is placed in accordance with parking signs and doesn't create a hazard for road users.

Assess the location according to the following restrictions, making sure none will apply during the time the skip will be placed on the road.

# Make sure the skip is NOT:

* in a Clearway
* in a No Stopping area
* in a Bus, Taxi or Permit Zone
* in a parking space reserved for people with disabilities
* in a bike lane
* on a footpath, nature strip, median strip or dividing strip
* within 20 metres of an intersection with traffic lights, or 10 metres of an intersection without traffic lights
* within 20 metres before and 10 metres after a school crossing, pedestrian crossing or bus stop
* within 10 metres of a tram safety zone or tram stop
* within 20 metres of a railway crossing
* in Bourke St Mall or Swanston St (between Flinders / La Trobe)
* in Lacey Pl, Bullens Ln, Calendonian Ln, Kirks Ln, Balcombe Pl, Albion Al or Carson Pl
* blocking a storm water channel
* impeding pedestrian access to a building
* impeding visibility for vehicles using a driveway or crossing
* exceeding the dimensions of a parking bay, or encroaching on the road or a bike lane
* in a laneway with less than 3 metres clearance for traffic after it has been placed.

For more information, contact City of Melbourne on 9658 9658 or [skipbinpermits@melbourne.vic.gov.au](mailto:skipbinpermits@melbourne.vic.gov.au)